**BROWARD COUNTY**

**UTILITY ENFORCEMENT SECTION**

**INDUSTRIAL PRETREATMENT PROGRAM- LOCAL LIMITS 2014**

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Maximum Concentration** | **Units** |
| Arsenic, Total | 0.10 | mg/L |
| BOD5 \* | 406 | mg/L |
| Cadmium, Total | 0.70 | mg/L |
| Chromium, Total | 1.0 | mg/L |
| Copper, Total | 2.0 | mg/L |
| Cyanide | 0.25 | mg/L |
| Iron, Total | 71.0 | mg/L |
| Lead, Total | 0.4 | mg/L |
| Mercury | 0.1 | mg/L |
| Nickel, Total | 1.8 | mg/L |
| Oil & Grease \* | 100 | mg/L |
| pH | 5.0-10.0 (+2.0) | S. U. |
| Silver, Total | 0.35 | mg/L |
| TSS\* | 400 | mg/L |
| Zinc, Total | 1.48 | mg/L |

\* These parameters may be surcharged.

For specific prohibitions, see Broward County Code Chapter 34, Article VI - Wastewater Discharge Standards, Section 34-139 (D). Copies are available from Broward County Water and Wastewater Services, Water and Wastewater Operations Division, Utility Enforcement Section. Telephone- (954) 831-3049.